Printdata Checklist

PDF Files must be ready to print and created as PDF/X4

Please do always create two PDF Files (equal quality) – once with a punching contour and once WITHOUT. Every font needs to be converted in paths. No different layers.

Everything you can see in the print file will be printed! The contour must **NOT be visible!**

**Colours / Fonts / Line strength / Resolution / Shape / cutting brands**

* Colour mode **CMYK**
* Grey objects (Fonts and lines) should always be created in default-black
* Fonts needs to be **converted in curves**
* Positive lines - **min. 1pt strength**
* Negative lines – **min. 3pt strength**
* **200dpi** for original image size (for huge motives correspondingly less). If the pictures resolution is less than 200dpi, the quality will be decreased.
* Safety distance for Logos, Codes, Textes, etc. (from boarders or fold lines) min. 5mm to rill and cut lines.
* Cutting and pass marks are essential to be situated outside the cutting brands
* Via filler /addition outer cutting brands **10mm**
* Cut marks (cross) size 20x20mm – Linestrenght 2pt

Every print file will be checked in terms of previously cited criteria. If some data files appear to be faulty or cannot be printed, you will receive an Information.

**Additional costs for repro performances**

Any reworking process or autocorrections for files which are not printable, incomplete or need to be revised, can be implemented within demand. The expanse will be charged with 110,- / hour.